**PRG\_22-14 IDTRONIC LEUZE RFID SYSTEMS**

**HF M30 IO-LINK DATASHEET**

Immagine che contiene connettore

Descrizione generata automaticamente

**RDH 142 00 M30**

|  |  |  |  |
| --- | --- | --- | --- |
| Version | Date | Author | Changelist |
| 01 | 06/09/2024 | Fabrizio Picotto | First release |

# Table of Contents

[1 Table of Contents 3](#_Toc176527815)

[2 Scope 4](#_Toc176527816)

[3 Field of Application 4](#_Toc176527817)

[4 Definitions and Abbreviations 4](#_Toc176527818)

[5 Technical Details 5](#_Toc176527819)

[6 Installation 7](#_Toc176527820)

[6.1 General Instructions 7](#_Toc176527821)

[6.2 Avoiding Interference 7](#_Toc176527822)

[6.3 Notes on Device Mounting 7](#_Toc176527823)

[6.4 Mechanical Design 8](#_Toc176527824)

[6.5 Notes on Tag Mounting 8](#_Toc176527825)

[6.6 Positioning of the Tags 8](#_Toc176527826)

[7 Connections 9](#_Toc176527827)

[7.1 Electrical Connections 9](#_Toc176527828)

[7.1.1 Power Supply Connection 9](#_Toc176527829)

[7.1.2 IO-Link Connection 10](#_Toc176527830)

[8 Status Display 11](#_Toc176527831)

[9 Antenna 12](#_Toc176527832)

[10 Maintenance, Repair and Disposal 13](#_Toc176527833)

[11 Mechanical Drawings 14](#_Toc176527834)

# Scope

This document refers to the Leuze HF Basic IO-Link device.

# Field of Application

This document applies to the device HF Basic IO-Link device with firmware version v1.0.0.

# Definitions and Abbreviations

| Term / Abbreviation | Definition |
| --- | --- |
| **TBD** | To Be Determined |
| **UID** | Unique Identifier |

# Technical Details

This section provides details on the technical data of the device.

| Electrical Data |  |
| --- | --- |
| Operating Voltage | Nominal 24 Vdc, range 18 … 36 Vdc |
| Power Ratings | 2 W |
| Protection Class | III |
| Operating Frequency | 13.56 MHz ±7 kHz |
| RFID Antenna | 1 × integrated |
| RFID Standard | ISO 15693, ISO 14443 A |

| Detection Zone |  |
| --- | --- |
| Distance Read Head Front | 60 mm[[1]](#footnote-2) |

| Interfaces |  |
| --- | --- |
| Communication Interface | IO-Link |

| Operating Conditions |  |
| --- | --- |
| Operating Temperature | -32 °C … +60 °C |
| Storage Temperature | -40 °C … +85 °C |
| Relative Humidity | Up to 95 %, non condensing |
| Degree of Protection | IP67 |

| Test / Approvals |  |
| --- | --- |
| Radio Approval for | USA, Canada, EU/RED |
| Shock Resistance | EN 60068-2-27, Test Ea  EN 60068-2-27, Test Eb |
| Vibration Resistance | EN 60068-2-6, Test Fc |

| Mechanical Data |  |
| --- | --- |
| Design | Cylindrical |
| Dimensions | M30 x 1.5 / L = 75.45mm |
| Net Weight | 120g |
| Housing Material | Metal, plastic |
| Housing Colour | Aluminium, RAL 9006  Red, RAL 3000 |
| Type of Fastening | Threaded M30 x 1.5 with locking nuts |

| Displays |  |
| --- | --- |
| Display | 1 × LED: bicolour green/red |

| Electrical Connections |  |
| --- | --- |
| Connector | 1 × 5-poles male M12 A-coded |

# Installation

## General Instructions

* Several devices installed next to each other interfere if they are not correctly configured.
* Installing a device in or on metal reduces the read and write distance.
* Keep the device away from direct sunlight, high humidity, extreme temperatures, and sources of electromagnetic interference. Any combination of these conditions might degrade performance or shorten the life of the device.
* Connect the device using a suitable cable as defined in electrical connections section.
* Power the device using a suitable external power supply as defined in electrical connections section. The boot sequence begins in either case when power is supplied to the device. This sequence typically completes within 5 seconds. After the boot sequence finishes, the device accepts commands, not before.

## Avoiding Interference

The device generates a modulated electrical field with a frequency of 13.56 MHz.

To avoid interference of the data communication:

* No other devices generating interference emission in this frequency band must be operated in its vicinity.
* Such devices are for example frequency converters and switched-mode power supplies.

If there are other devices in the same frequency band in the vicinity:

* The mounting distances between the devices should be as large as possible.
* Use the devices in alternating operation.
* Switch the HF field of the device on/off.

## Notes on Device Mounting

For installation:

* Use the supplied nuts to fix the device to a plastic or metal panel.

## Mechanical Design

|  |  |
| --- | --- |
| Immagine che contiene disegno, schizzo, illustrazione, design  Descrizione generata automaticamente  3  2  4  1 | 1. Status display 2. Electrical connections 3. Sensing element 4. Mounting nuts |

## Notes on Tag Mounting

* For installation in and on metal tags provided for this purpose must be used.
* The tag must be placed in the reading area of the device antenna. The angle of aperture and the operating distance must be adhered to.
* The orientation of the device antenna axis must correspond with the axis of the tag for best performance.

## Positioning of the Tags

|  |  |
| --- | --- |
| Immagine che contiene schizzo, bianco e nero, schermata, arte  Descrizione generata automaticamente | * Align the tag on the antenna central axis. * The distance “D” is indicated in the “Antenna” section. |

# Connections

This section provides details on the connections of the device.


Observe the following instructions before electrical installation.

|  |  |
| --- | --- |
| Immagine che contiene Segnale stradale, triangolo, giallo, cartello  Descrizione generata automaticamente | * The device must be connected by a skilled qualified person. * Device of protection class III. * Electric supply via PELV/SELV circuits only. * Disconnect power before connecting the device. * Connect the device according to the indicated pin connection. |

## Electrical Connections

### Power Supply Connection

The power supply connection is designed as a 5-poles male M12 A-coded connector. This connector is shared with IO-Link interface.




| Pin | No | Description | DIN47100 Wire Cable Colour |
| --- | --- | --- | --- |
| VCC | 1 | DC power supply, VCC | Brown |
| DI/DO | 2 | Not used | White |
| GND | 3 | DC power supply return path, GND | Blue |
| C/Q | 4 | IO-Link | Black |
| NC | 5 | Not Connected | Grey |

|  |  |
| --- | --- |
| Immagine che contiene strumento di scrittura, forniture per ufficio, cancelleria, Strumenti per contrassegnare  Descrizione generata automaticamente | To ensure interference-free operation, the device must be connected to an earth potential free from external voltage. |

### IO-Link Connection

The serial IO-Link interface connection is designed as a 5-poles male M12 A-coded connector. This connector is shared with power supply.



| Pin | No | Description | DIN47100 Wire Cable Colour |
| --- | --- | --- | --- |
| VCC | 1 | DC power supply, VCC | Brown |
| DI/DO | 2 | Not used | White |
| GND | 3 | DC power supply return path, GND | Blue |
| C/Q | 4 | IO-Link | Black |
| NC | 5 | Not Connected | Grey |

|  |  |
| --- | --- |
| Immagine che contiene strumento di scrittura, forniture per ufficio, cancelleria, Strumenti per contrassegnare  Descrizione generata automaticamente | To ensure interference-free operation, the device must be connected to an earth potential free from external voltage. |

# Status Display

This section provides details on the status display of the device.

| Colour | State | Meaning |
| --- | --- | --- |
| (red) | Static on | * System error * System initialization |
| (green) | Static on | * Device ready, antenna not active |
| (yellow) | Blinking 4 Hz | * Antenna active, tag detected |
| (yellow) | Static on | * Antenna active, no tag detected |
| (off) | Static off | * Power supply is missing * Hardware defect |

# Antenna

This section provides details on the antenna of the device.

The device integrates the RFID antenna inside the case.

The read range of an RFID system always depends on various factors like antenna size, transponder size, transponder IC type, orientation between transponder and reader antenna, position of the transponder versus the reader antenna, noise environment, metallic environment, etc. Therefore, all data about read ranges can only be typical values measured under laboratory conditions. In real live applications the read range may differ from the data mentioned in the datasheet.

| Detection Zone |  |
| --- | --- |
| Distance Read Head Front | <60mm, referred to a 50x50mm white label tag, IC NXP ICODE SLIX2 |
| Distance Read Head Side | <60mm, referred to a 50x50mm white label tag, IC NXP ICODE SLIX2 |

# Maintenance, Repair and Disposal

If used correctly, no maintenance and repair measures are necessary

* The device must only be repaired by the manufacturer.
* After use dispose of the device in an environmentally friendly way in accordance with the applicable national regulations.
* Keep the device free from soiling.

# Mechanical Drawings

Immagine che contiene schizzo, testo, disegno, diagramma

Descrizione generata automaticamente

Dimensions in mm.

1. Reading distance depends on transponder type, antenna and environmental conditions. [↑](#footnote-ref-2)